{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":50,"n_cols":4,"rows_kept":50,"merged":[[0,0,0,3],[4,0,4,3],[30,0,34,0],[30,1,34,1],[30,3,34,3],[35,0,40,0],[35,1,40,1],[35,3,40,3],[41,0,43,0],[41,1,43,1],[41,3,43,3],[47,1,49,1]]}
["豪美模具中心双室油淬炉技术要求"]
["设备维修主管：",null,"模具中心生产部经理："]
["设备部总监：",null,"模具中心总监："]
["序号","项目名称","参数要求","评标分类"]
["一、机床"]
[1,"有效工作区尺寸","1500（L）×800（W）×800（H）","标配"]
[2,"最大装炉量","2000 kg","标配"]
[3,"加热功率","300 Kw","标配"]
[4,"最高温度","1320℃","标配"]
[5,"工作温度","550℃～1270℃","标配"]
[6,"温度均匀性","≤±5℃（550℃～1050℃，空炉真空状态测量）","标配"]
[7,"分压范围","10～500 Pa","标配"]
[8,"压升率","0.65 Pa/h","标配"]
[9,"抽速","从105Pa抽至5Pa小于30min（空炉、充分烘炉后回充高纯氮气冷态下）","标配"]
[10,"升温速率","室温升至1100℃小于60min（空炉）","标配"]
[11,"气冷压强","1.99bar","标配"]
[12,"控温精度","≤±1.0℃","标配"]
[13,"炉壁外温度","＜室温+25℃","标配"]
[14,"极限真空度","4×10-1 Pa","标配"]
[15,"升降机构","通过滚珠丝杠机构带动升降料车","标配"]
[16,"炉外料车","电动","标配"]
[17,"进出料机构","双拨杆结构，变频器控制","标配"]
[18,"保温材料","石墨毡和陶瓷纤维毡","标配"]
[19,"油冷却装置","通过管道与油槽连接，加快油冷的速度","标配"]
[20,"真空机组","配两套真空机组，具有互通性","标配"]
[21,"温控仪表","欧陆2604或同级别","标配"]
[22,"记录仪","杭州盘古KT500系列12通道","标配"]
[23,"稳压器","保证电控柜仪器仪表电源稳定","标配"]
[24,"真空仪","成都正华ZDR系列","标配"]
["二、通用要求"]
[1,"电气控制","①电箱配有足够的散热器和鲜风口，防护等级IP46。","标配"]
[null,null,"②电箱与机器本体最好独立分开，如不能独立分开需有防振动措施。"]
[null,null,"③走线布管美观，采用线管+管码固定，固定牢固，横平竖直。"]
[null,null,"④按钮及线码标识清晰，电箱贴“小心触电”警示标识。"]
[null,null,"⑤其他危险部位(含转动)陪有便于拆装的护罩(套)并贴有相应警示标识。"]
[2,"电气元件","①元件：施耐德。","标配"]
[null,null,"②PLC:西门子S7-1500或三菱3U系列(带以太网接口)。"]
[null,null,"③触摸屏：威纶通或昆仑通态。"]
[null,null,"④变频器：三菱或力士乐。"]
[null,null,"④所有电机均符合YE3或YE4国家节能要求。"]
[]
[3,"气动",null,"标配"]
[null,null,"设备需用压缩空气必须配置气动三联件。"]
[null,null,"所有气动原件(汽缸、阀、三联件等)品牌参考我司品牌库要求(亚德客、SMC),并配置消声器。"]
["三、其它要求"]
[null,"企业注册资金","≥1500万元","并附带同行业销售案例"]
[null,"售后服务","24小时内响应到厂"]
[null,"配件要求","配料框底板一套（2个料框1件底板）","料框材质为2520高温不锈钢一体铸造"]
[null,null,"配高温室石墨支架一套","只需配承重部分支架及易损零件"]
[null,null,"配对应容量1号真空淬火油","200L/桶约45-50桶"]